**root教程**

1. 固件需升级到V1.1.0.12及以后版本，升级完毕后会自动重启

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

1. 开启 root

注意：如果需要 root 必须同意免责条款，否则机器不会开启 ssh 服务

注意：root 后可能会造成机器相关功能故障，请谨慎使用

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

**翻译：**

**Root Tutorial**

1. The firmware needs to be upgraded to version V1.1.0.12 or later. After the upgrade is completed, it will automatically reboot.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

1. Enable Root

Note: If root access is required, you must agree to the disclaimer, otherwise the machine will not initiate the SSH service.

Note: Rooting may cause malfunction of certain features in the machine. Please use it with caution.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |